

|  |  |
| --- | --- |
| **CHAIR TYPE:** | **Quantity Required:**  **23** |
| ROTARY CHAIR  ROTARY STOOL |
| **Instructions to Users:**   * Choose the attributes (🡪) that must be included for your requirement. Use 1 builder per type of chair. * *Note: if more than 1* “” *is chosen then all attributes will be considered acceptable for the requirement.* | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Criteria** | | **Requirement Choices** | | | | *Annex A*  *reference:* |
| *Environmental* | | *All products meet a minimum of ANSI/BIFMA e3 minimum Level® 2*  *All plastic components are recyclable at the end of their life.* | | | | *1.2.8* |
| *Weight Capacity* | | Standard *(up to 275 lbs)*  Large-occupant *(275+ lbs up to 400 lbs)* | | | | *1.5.7* |
| *Usage* | | Single shift  24/7 *(3 continuous working shifts, 7 days a week)* | | | | *1.5.2*  *1.7.1.3* |
| **A** | *Headrest* | No  Yes *(adjustable)*  *No preference* | | | | *2.1.13* |
| **B** | *Backrest Height* | Standard  High  *No preference* | | | | *2.1.7* |
| **C** | *Lumbar Support* | Fixed position  Adjustable *(by user)*  Self-Adjusting mechanism  *No preference* | | | | *2.1.6* |
| **D** | *Armrests* | Adjustable | Height Adjustment  Lateral Adjustment  Fully Articulating | *Armrest Style:* | | *2.1.10* |
| T-arm (DD) | Fixed  *Adjustable* |
| Cantilever | |
| Fixed | | T-arm  Cantilever  Loop  *No preference* | |
| **E** | *Seat Depth* | Adjustable | | | | *2.1.2* |
| Fixed position | Shallow  Medium  Deep | | |
| **F** | *Seat Width* | *Standard based on weight capacity chosen above* | | | | *2.1.3*  *2.2.2* |
| **G** | *Seat Height* | *Rotary Chair* | Adjustable – standard range  Adjustable - low range | | | *2.1.4* |
| *Rotary Stool* | *Adjustable* | | |
| **H** | *Tilt Mechanism* | *Rotary Chair* | Multifunction  Synchro Tilt  Unison Tilt  Weight Sensitive  *No preference* | | | *1.5.11*  *2.1.8* |
| *Rotary Stool* | Multifunction  Synchro Tilt  Unison Tilt  Weight Sensitive  Fixed Back  *No preference* | | |
| **I** | *Seat Angle and Backrest-to-seat Angle* | Adjustable and lockable *(not applicable to weight sensitive tilt mechanisms)* | | | | *2.1.5*  *2.1.9* |
| **J** | *Casters* | *for use on:*  carpet  hard surfaces | | | | *2.1.11* |
| **L** | *Footrest*  *(rotary stools only)* | integrated fixed height  adjustable height | | | | *2.1.12* |
| *Finishes* | | Backrest: | Upholstery  Non-upholstery *(ie. flexible plastic)*  Mesh Material | | | *2.1.15* |
| Seat: | Upholstery  Non-upholstery *(ie. flexible plastic*)  Mesh Material | | |
| Base Frame: | Metal  Plastic | | |
| *Labelling and Instructions* | | *All chairs must be provided with labelling and instructions* | | | | *1.3.2* |
| *Accessibility* | | *Not applicable*  Adjustment levers to be equipped with brail | | | | *1.6.3* |
| *Additional Criteria* | | * *Please include some blue colour tones for the seat upholstery options* * *Please provide a photo representations of products being offered with your bid submission.* | | | | |

|  |  |
| --- | --- |
| **CHAIR TYPE** | **Quantity Required:**  **10** |
| SIDE CHAIR  ROTARY GUEST CHAIR |
| ***Instructions to Users:***   * *Choose the attributes* (🡪) *that must be included for your requirement. Use 1 builder per type of chair.* * *Note: if more than 1* “” *is chosen then all attributes will be considered acceptable for the requirement.* | |





*Side Chair Rotary Guest Chair*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Criteria** | | **Requirement Choices** | | | *Annex A*  *reference:* |
| *Environmental* | | *All products meet a minimum of ANSI/BIFMA e3 minimum Level® 2*  *All plastic components are recyclable at the end of their life.* | | | *1.2.8* |
| **B** | *Backrest Height* | *Standard as fixed based on chair type chosen above* | | | *2.3.7*  *2.3.8* |
| **C** | *Lumbar Support* | Yes *(fixed position)*  No  *No preference* | | | *2.3.6* |
| **D** | *Armrests* | Yes *(fixed position)* | *Style:*  Cantilever  T-arm  Closed or Loop  *No preference* | | *2.3.10* |
| No | | |
| **E &F** | *Seat Width & Depth* | *Standard as fixed* | | | *2.3.2* |
| **G** | *Seat Height* | Fixed *(side chair OR rotary guest chair)*  Height Adjustable *(rotary guest chair only)* | | | *2.3.3* |
| **H** | *Leg Support* | Side Chair:  4 Post Legs  Cantilever  Sled | | Glides  Casters | *2.3.11* |
| Rotary Guest Chair:  4 star base  5 star base | | Glides  Casters |
| **I** | *Backrest-to-seat Angle* | *Fixed angle* | | | *2.3.9* |
| *Seat Angle*  *(rotary guest chair only)* | Fixed  Adjustable with tilt mechanism | | | *2.3.4* |
| *Stacking* | | Stacking *(vertical)*   Nesting *(horizontal)*  Non-stacking  *No preference* | | | *2.3.12* |
| *Finishes* | | Backrest: | Upholstery  Wood  Plastic  Mesh  Other: *(specify)* | | *2.3.13* |
| Seat: | Upholstery  Wood  Plastic  Mesh  Other: *(specify)* | |
| Base Frame: | Plastic  Wood  Metal *( ie. wired)* | |
| *Additional Criteria* | | * *Please include some blue colour tones for the seat upholstery options* * *Please provide a photo representations of products being offered with your bid submission.* | | | |