

|  |  |
| --- | --- |
| **CHAIR TYPE:** | **Quantity Required: \_\_\_\_\_\_** |
| ROTARY CHAIR  ROTARY STOOL |
| **Instructions to Users:**   * Choose the attributes (🡪) that must be included for your requirement. Use 1 builder per type of chair. * *Note: if more than 1* “” *is chosen then all attributes will be considered acceptable for the requirement.* | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Criteria** | | **Requirement Choices** | | | | *Annex A*  *reference:* |
| *Environmental* | | *All products meet a minimum of ANSI/BIFMA e3 minimum Level® 2*  *All plastic components are recyclable at the end of their life.* | | | | *1.2.8* |
| *Weight Capacity* | | Standard *(up to 275 lbs)*  Large-occupant *(275+ lbs up to 400 lbs)* | | | | *1.5.7* |
| *Usage* | | Single shift  24/7 *(3 continuous working shifts, 7 days a week)* | | | | *1.5.2*  *1.7.1.3* |
| **A** | *Headrest* | No  Yes *(adjustable)*  *No preference* | | | | *2.1.13* |
| **B** | *Backrest Height* | Standard  High  *No preference* | | | | *2.1.7* |
| **C** | *Lumbar Support* | Fixed position  Adjustable *(by user)*  Self-Adjusting mechanism  *No preference* | | | | *2.1.6* |
| **D** | *Armrests* | Adjustable | Height Adjustment  Lateral Adjustment  Fully Articulating | *Armrest Style:* | | *2.1.10* |
| T-arm (DD) | Fixed  *Adjustable* |
| Cantilever | |
| Fixed | | T-arm  Cantilever  Loop  *No preference* | |
| **E** | *Seat Depth* | Adjustable | | | | *2.1.2* |
| Fixed position | Shallow  Medium  Deep | | |
| **F** | *Seat Width* | *Standard based on weight capacity chosen above* | | | | *2.1.3*  *2.2.2* |
| **G** | *Seat Height* | *Rotary Chair* | Adjustable – standard range  Adjustable - low range | | | *2.1.4* |
| *Rotary Stool* | *Adjustable* | | |
| **H** | *Tilt Mechanism* | *Rotary Chair* | Multifunction  Synchro Tilt  Unison Tilt  Weight Sensitive  *No preference* | | | *1.5.11*  *2.1.8* |
| *Rotary Stool* | Multifunction  Synchro Tilt  Unison Tilt  Weight Sensitive  Fixed Back  *No preference* | | |
| **I** | *Seat Angle and Backrest-to-seat Angle* | Adjustable and lockable *(not applicable to weight sensitive tilt mechanisms)* | | | | *2.1.5*  *2.1.9* |
| **J** | *Casters* | *for use on:*  carpet  hard surfaces | | | | *2.1.11* |
| **L** | *Footrest*  *(rotary stools only)* | integrated fixed height  adjustable height | | | | *2.1.12* |
| *Finishes* | | Backrest: | Upholstery  Non-upholstery *(ie. flexible plastic)*  Mesh Material | | | *2.1.15* |
| Seat: | Upholstery  Non-upholstery *(ie. flexible plastic*)  Mesh Material | | |
| Base Frame: | Metal  Plastic | | |
| *Labelling and Instructions* | | *All chairs must be provided with labelling and instructions* | | | | *1.3.2* |
| *Accessibility* | | *Not applicable*  Adjustment levers to be equipped with brail | | | | *1.6.3* |
| *Additional Criteria* | | * *Additional Criteria must be generic,* ***not*** *Supplier specific and cannot contradict the RFSA Technical Specifications @ Annex A.* * *May also request additional information such as photo representations of products being offered or inclusion of specific colour tones or listing of finish offerings available to be provided prior to contract award.* | | | | |

|  |  |
| --- | --- |
| **CHAIR TYPE** | **Quantity Required:**  **\_\_\_\_\_\_\_** |
| SIDE CHAIR  ROTARY GUEST CHAIR |
| ***Instructions to Users:***   * *Choose the attributes* (🡪) *that must be included for your requirement. Use 1 builder per type of chair.* * *Note: if more than 1* “” *is chosen then all attributes will be considered acceptable for the requirement.* | |





*Side Chair Rotary Guest Chair*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Criteria** | | **Requirement Choices** | | | *Annex A*  *reference:* |
| *Environmental* | | *All products meet a minimum of ANSI/BIFMA e3 minimum Level® 2*  *All plastic components are recyclable at the end of their life.* | | | *1.2.8* |
| **B** | *Backrest Height* | *Standard as fixed based on chair type chosen above* | | | *2.3.7*  *2.3.8* |
| **C** | *Lumbar Support* | Yes *(fixed position)*  No  *No preference* | | | *2.3.6* |
| **D** | *Armrests* | Yes *(fixed position)* | *Style:*  Cantilever  T-arm  Closed or Loop  *No preference* | | *2.3.10* |
| No | | |
| **E &F** | *Seat Width & Depth* | *Standard as fixed* | | | *2.3.2* |
| **G** | *Seat Height* | Fixed *(side chair OR rotary guest chair)*  Height Adjustable *(rotary guest chair only)* | | | *2.3.3* |
| **H** | *Leg Support* | Side Chair:  4 Post Legs  Cantilever  Sled | | Glides  Casters | *2.3.11* |
| Rotary Guest Chair:  4 star base  5 star base | | Glides  Casters |
| **I** | *Backrest-to-seat Angle* | *Fixed angle* | | | *2.3.9* |
| *Seat Angle*  *(rotary guest chair only)* | Fixed  Adjustable with tilt mechanism | | | *2.3.4* |
| *Stacking* | | Stacking *(vertical)*   Nesting *(horizontal)*  Non-stacking  *No preference* | | | *2.3.12* |
| *Finishes* | | Backrest: | Upholstery  Wood  Plastic  Mesh  Other: *(specify)* | | *2.3.13* |
| Seat: | Upholstery  Wood  Plastic  Mesh  Other: *(specify)* | |
| Base Frame: | Plastic  Wood  Metal *( ie. wired)* | |
| *Additional Criteria* | | * *Additional Criteria must be generic,* ***not*** *Supplier specific and cannot contradict the RFSA Technical Specifications @ Annex A.* * *Specify here if a storage trolly must also be provided with product.* * *May also request additional information such as photo representations of products being offered or inclusion of specific colour tones or listing of finish offerings available to be provided prior to contract award.* | | | |